#

##

##

    µVision Build Log
    Project:
    C:\Users\Administrator\Desktop\TX\Project\Project.uvproj
    Project File Date:  02/08/2017

    Output:
    Build target 'PROJECT'
    linking...
    ..\Output\Project.axf: Error: L6218E: Undefined symbol NRF24L01_Check (referred from main.o).
    ..\Output\Project.axf: Error: L6218E: Undefined symbol NRF24L01_Init (referred from main.o).
    ..\Output\Project.axf: Error: L6218E: Undefined symbol NRF24L01_TxPacket (referred from main.o).
    ..\Output\Project.axf: Error: L6218E: Undefined symbol TX_Mode (referred from main.o).
    "..\Output\Project.axf" - 4 Errors, 0 Warning(s).
    Target not created
    Build target 'PROJECT'
    linking...
    ..\Output\Project.axf: Error: L6218E: Undefined symbol NRF24L01_Check (referred from main.o).
    ..\Output\Project.axf: Error: L6218E: Undefined symbol NRF24L01_Init (referred from main.o).
    ..\Output\Project.axf: Error: L6218E: Undefined symbol NRF24L01_TxPacket (referred from main.o).
    ..\Output\Project.axf: Error: L6218E: Undefined symbol TX_Mode (referred from main.o).
    "..\Output\Project.axf" - 4 Errors, 0 Warning(s).
    Target not created
    Build target 'PROJECT'
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling misc.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_cec.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling delay.c...
    compiling bsp_NVIC.C...
    compiling bsp_iic.c...
    compiling bsp_GPIO.c...
    compiling bsp_usart.c...
    compiling 24cxx.c...
    compiling oled.c...
    compiling 24l01.c...
    ..\HARDWARE\24L01\24l01.c(3): error:  #5: cannot open source input file "bsp_spi.h": No such file or directory
    compiling main.c...
    compiling stm32f10x_it.c...
    "..\Output\Project.axf" - 1 Errors, 0 Warning(s).
    Target not created
    Build target 'PROJECT'
    compiling core_cm3.c...
    compiling system_stm32f10x.c...
    compiling misc.c...
    compiling stm32f10x_adc.c...
    compiling stm32f10x_bkp.c...
    compiling stm32f10x_can.c...
    compiling stm32f10x_cec.c...
    compiling stm32f10x_crc.c...
    compiling stm32f10x_dac.c...
    compiling stm32f10x_dbgmcu.c...
    compiling stm32f10x_dma.c...
    compiling stm32f10x_exti.c...
    compiling stm32f10x_flash.c...
    compiling stm32f10x_fsmc.c...
    compiling stm32f10x_gpio.c...
    compiling stm32f10x_i2c.c...
    compiling stm32f10x_iwdg.c...
    compiling stm32f10x_pwr.c...
    compiling stm32f10x_rcc.c...
    compiling stm32f10x_rtc.c...
    compiling stm32f10x_sdio.c...
    compiling stm32f10x_spi.c...
    compiling stm32f10x_tim.c...
    compiling stm32f10x_usart.c...
    compiling stm32f10x_wwdg.c...
    compiling delay.c...
    compiling bsp_NVIC.C...
    compiling bsp_iic.c...
    compiling bsp_GPIO.c...
    compiling bsp_usart.c...
    compiling bsp_spi.c...
    compiling 24cxx.c...
    compiling oled.c...
    compiling 24l01.c...
    compiling main.c...
    compiling stm32f10x_it.c...
    linking...
    Program Size: Code=11120 RO-data=2364 RW-data=964 ZI-data=1908
    FromELF: creating hex file...
    "..\Output\Project.axf" - 0 Errors, 0 Warning(s).
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'PROJECT'
    compiling 24l01.c...
    compiling main.c...
    linking...
    Program Size: Code=11116 RO-data=2364 RW-data=964 ZI-data=1908
    FromELF: creating hex file...
    "..\Output\Project.axf" - 0 Errors, 0 Warning(s).
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'PROJECT'
    compiling main.c...
    ..\User\main.c(40): warning:  #177-D: variable "tmp" was declared but never referenced
    linking...
    Program Size: Code=11012 RO-data=2364 RW-data=964 ZI-data=1908
    FromELF: creating hex file...
    "..\Output\Project.axf" - 0 Errors, 1 Warning(s).
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'PROJECT'
    compiling main.c...
    ..\User\main.c(40): warning:  #177-D: variable "tmp" was declared but never referenced
    linking...
    Program Size: Code=11008 RO-data=2364 RW-data=964 ZI-data=1908
    FromELF: creating hex file...
    "..\Output\Project.axf" - 0 Errors, 1 Warning(s).
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'PROJECT'
    compiling main.c...
    ..\User\main.c(40): warning:  #177-D: variable "tmp" was declared but never referenced
    ..\User\main.c(42): warning:  #177-D: variable "p" was declared but never referenced
    linking...
    Program Size: Code=6914 RO-data=2342 RW-data=952 ZI-data=1632
    FromELF: creating hex file...
    "..\Output\Project.axf" - 0 Errors, 2 Warning(s).
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'PROJECT'
    compiling main.c...
    ..\User\main.c(42): warning:  #177-D: variable "p" was declared but never referenced
    linking...
    Program Size: Code=8746 RO-data=2350 RW-data=952 ZI-data=1656
    FromELF: creating hex file...
    "..\Output\Project.axf" - 0 Errors, 1 Warning(s).
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'PROJECT'
    compiling main.c...
    ..\User\main.c(42): warning:  #177-D: variable "p" was declared but never referenced
    linking...
    Program Size: Code=8750 RO-data=2350 RW-data=952 ZI-data=1656
    FromELF: creating hex file...
    "..\Output\Project.axf" - 0 Errors, 1 Warning(s).
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Build target 'PROJECT'
    compiling main.c...
    linking...
    Program Size: Code=8806 RO-data=2350 RW-data=952 ZI-data=1688
    FromELF: creating hex file...
    "..\Output\Project.axf" - 0 Errors, 0 Warning(s).
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...
    Load "..\\Output\\Project.axf"
    Set JLink Project File to "C:\Users\Administrator\Desktop\TX\Project\JLinkSettings.ini"
    * JLink Info: Device "STM32F103C8" selected (64 KB flash, 20 KB RAM).

    JLink info:
    ------------
    DLL: V4.90 , compiled Jul 28 2014 10:35:20
    Firmware: J-Link ARM-OB STM32 compiled Aug 22 2012 19:52:04
    Hardware: V7.00
    S/N : 20090928
    Feature(s) : RDI,FlashDL,FlashBP,JFlash,GDBFull

    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found SWD-DP with ID 0x1BA01477
    * JLink Info: Found Cortex-M3 r1p1, Little endian.
    * JLink Info: FPUnit: 6 code (BP) slots and 2 literal slots
    * JLink Info: TPIU fitted.
    * JLink Info: ETM fitted.
    ROMTableAddr = 0xE00FF003

    Target info:
    ------------
    Device: STM32F103C8
    VTarget = 3.300V
    State of Pins:
    TCK: 0, TDI: 0, TDO: 1, TMS: 0, TRES: 1, TRST: 1
    Hardware-Breakpoints: 6
    Software-Breakpoints: 8192
    Watchpoints:          4
    JTAG speed: 1000 kHz

    Erase Done.
    Programming Done.
    Verify OK.
    Application running ...